--altsyncram CBX_DECLARE_ALL_CONNECTED_PORTS="OFF" CYCLONEII_M4K_COMPATIBILITY="ON" DEVICE_FAMILY="Cyclone II" INIT_FILE="single_cycle_datapath0.rtl.mif" LOW_POWER_MODE="AUTO" NUMWORDS_A=64 OPERATION_MODE="ROM" OUTDATA_REG_A="UNREGISTERED" RAM_BLOCK_TYPE="AUTO" WIDTH_A=28 WIDTHAD_A=6 address_a clock0 q_a CARRY_CHAIN="MANUAL" CARRY_CHAIN_LENGTH=48
--VERSION_BEGIN 6.1 cbx_altsyncram 2006:11:03:10:29:54:SJ cbx_cycloneii 2006:09:29:19:03:26:SJ cbx_lpm_add_sub 2006:10:10:22:03:24:SJ cbx_lpm_compare 2006:04:25:14:54:12:SJ cbx_lpm_decode 2006:04:25:15:10:18:SJ cbx_lpm_mux 2006:04:25:15:10:08:SJ cbx_mgl 2006:10:27:16:08:48:SJ cbx_stratix 2006:09:18:10:47:42:SJ cbx_stratixii 2006:10:13:14:01:30:SJ cbx_stratixiii 2006:10:19:19:28:28:SJ cbx_util_mgl 2006:11:03:10:32:30:SJ  VERSION_END


--  Copyright (C) 1991-2006 Altera Corporation
--  Your use of Altera Corporation's design tools, logic functions 
--  and other software and tools, and its AMPP partner logic 
--  functions, and any output files from any of the foregoing 
--  (including device programming or simulation files), and any 
--  associated documentation or information are expressly subject 
--  to the terms and conditions of the Altera Program License 
--  Subscription Agreement, Altera MegaCore Function License 
--  Agreement, or other applicable license agreement, including, 
--  without limitation, that your use is for the sole purpose of 
--  programming logic devices manufactured by Altera and sold by 
--  Altera or its authorized distributors.  Please refer to the 
--  applicable agreement for further details.


PARAMETERS
(
	PORT_A_ADDRESS_WIDTH = 1,
	PORT_A_BYTE_ENABLE_MASK_WIDTH = 1,
	PORT_A_DATA_WIDTH = 1,
	PORT_B_ADDRESS_WIDTH = 1,
	PORT_B_BYTE_ENABLE_MASK_WIDTH = 1,
	PORT_B_DATA_WIDTH = 1
);
FUNCTION cycloneii_ram_block (clk0, clk1, clr0, clr1, ena0, ena1, portaaddr[PORT_A_ADDRESS_WIDTH-1..0], portaaddrstall, portabyteenamasks[PORT_A_BYTE_ENABLE_MASK_WIDTH-1..0], portadatain[PORT_A_DATA_WIDTH-1..0], portawe, portbaddr[PORT_B_ADDRESS_WIDTH-1..0], portbaddrstall, portbbyteenamasks[PORT_B_BYTE_ENABLE_MASK_WIDTH-1..0], portbdatain[PORT_B_DATA_WIDTH-1..0], portbrewe)
WITH ( 	CONNECTIVITY_CHECKING,	DATA_INTERLEAVE_OFFSET_IN_BITS,	DATA_INTERLEAVE_WIDTH_IN_BITS,	DONT_POWER_OPTIMIZE,	INIT_FILE,	INIT_FILE_LAYOUT,	init_file_restructured,	LOGICAL_RAM_NAME,	mem_init0,	mem_init1,	MIXED_PORT_FEED_THROUGH_MODE,	OPERATION_MODE,	PORT_A_ADDRESS_WIDTH,	PORT_A_BYTE_ENABLE_MASK_WIDTH,	PORT_A_BYTE_SIZE,	PORT_A_DATA_OUT_CLEAR,	PORT_A_DATA_OUT_CLOCK,	PORT_A_DATA_WIDTH,	PORT_A_DISABLE_CE_ON_INPUT_REGISTERS,	PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS,	PORT_A_FIRST_ADDRESS,	PORT_A_FIRST_BIT_NUMBER,	PORT_A_LAST_ADDRESS,	PORT_A_LOGICAL_RAM_DEPTH,	PORT_A_LOGICAL_RAM_WIDTH,	PORT_B_ADDRESS_CLOCK,	PORT_B_ADDRESS_WIDTH,	PORT_B_BYTE_ENABLE_CLOCK,	PORT_B_BYTE_ENABLE_MASK_WIDTH,	PORT_B_BYTE_SIZE,	PORT_B_DATA_IN_CLOCK,	PORT_B_DATA_OUT_CLEAR,	PORT_B_DATA_OUT_CLOCK,	PORT_B_DATA_WIDTH,	PORT_B_DISABLE_CE_ON_INPUT_REGISTERS,	PORT_B_DISABLE_CE_ON_OUTPUT_REGISTERS,	PORT_B_FIRST_ADDRESS,	PORT_B_FIRST_BIT_NUMBER,	PORT_B_LAST_ADDRESS,	PORT_B_LOGICAL_RAM_DEPTH,	PORT_B_LOGICAL_RAM_WIDTH,	PORT_B_READ_ENABLE_WRITE_ENABLE_CLOCK,	POWER_UP_UNINITIALIZED,	RAM_BLOCK_TYPE,	SAFE_WRITE) 
RETURNS ( portadataout[PORT_A_DATA_WIDTH-1..0], portbdataout[PORT_B_DATA_WIDTH-1..0]);

--synthesis_resources = M4K 1 
OPTIONS ALTERA_INTERNAL_OPTION = "OPTIMIZE_POWER_DURING_SYNTHESIS=NORMAL_COMPILATION";

SUBDESIGN altsyncram_b301
( 
	address_a[5..0]	:	input;
	clock0	:	input;
	q_a[27..0]	:	output;
) 
VARIABLE 
	ram_block1a0 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 0,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a1 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 1,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a2 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 2,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a3 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 3,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a4 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 4,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a5 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 5,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a6 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 6,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a7 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 7,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a8 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 8,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a9 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 9,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a10 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 10,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a11 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 11,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a12 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 12,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a13 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 13,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a14 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 14,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a15 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 15,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a16 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 16,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a17 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 17,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a18 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 18,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a19 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 19,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a20 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 20,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a21 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 21,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a22 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 22,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a23 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 23,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a24 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 24,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a25 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 25,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a26 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 26,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block1a27 : cycloneii_ram_block
		WITH (
			CONNECTIVITY_CHECKING = "OFF",
			INIT_FILE = "single_cycle_datapath0.rtl.mif",
			INIT_FILE_LAYOUT = "port_a",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			OPERATION_MODE = "rom",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_OUT_CLEAR = "none",
			PORT_A_DATA_OUT_CLOCK = "none",
			PORT_A_DATA_WIDTH = 1,
			PORT_A_DISABLE_CE_ON_INPUT_REGISTERS = "off",
			PORT_A_DISABLE_CE_ON_OUTPUT_REGISTERS = "off",
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 27,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 28,
			RAM_BLOCK_TYPE = "AUTO"
		);
	address_a_wire[5..0]	: WIRE;

BEGIN 
	ram_block1a[27..0].clk0 = clock0;
	ram_block1a[27..0].portaaddr[] = ( address_a_wire[5..0]);
	address_a_wire[] = address_a[];
	q_a[] = ( ram_block1a[27..0].portadataout[0..0]);
END;
--VALID FILE
