/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/
/*
Copyright (C) 1991-2006 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.
*/
(header "symbol" (version "1.1"))
(symbol
	(rect 16 16 296 240)
	(text "datapath" (rect 5 0 47 12)(font "Arial" ))
	(text "inst" (rect 8 208 25 220)(font "Arial" ))
	(port
		(pt 0 32)
		(input)
		(text "instruction[31..0]" (rect 0 0 82 12)(font "Arial" ))
		(text "instruction[31..0]" (rect 21 27 103 39)(font "Arial" ))
		(line (pt 0 32)(pt 16 32)(line_width 3))
	)
	(port
		(pt 0 48)
		(input)
		(text "mem_read_data[31..0]" (rect 0 0 110 12)(font "Arial" ))
		(text "mem_read_data[31..0]" (rect 21 43 131 55)(font "Arial" ))
		(line (pt 0 48)(pt 16 48)(line_width 3))
	)
	(port
		(pt 0 64)
		(input)
		(text "RegDst" (rect 0 0 37 12)(font "Arial" ))
		(text "RegDst" (rect 21 59 58 71)(font "Arial" ))
		(line (pt 0 64)(pt 16 64)(line_width 1))
	)
	(port
		(pt 0 80)
		(input)
		(text "Jump" (rect 0 0 27 12)(font "Arial" ))
		(text "Jump" (rect 21 75 48 87)(font "Arial" ))
		(line (pt 0 80)(pt 16 80)(line_width 1))
	)
	(port
		(pt 0 96)
		(input)
		(text "Branch" (rect 0 0 34 12)(font "Arial" ))
		(text "Branch" (rect 21 91 55 103)(font "Arial" ))
		(line (pt 0 96)(pt 16 96)(line_width 1))
	)
	(port
		(pt 0 112)
		(input)
		(text "MemtoReg" (rect 0 0 53 12)(font "Arial" ))
		(text "MemtoReg" (rect 21 107 74 119)(font "Arial" ))
		(line (pt 0 112)(pt 16 112)(line_width 1))
	)
	(port
		(pt 0 128)
		(input)
		(text "ALUop[1..0]" (rect 0 0 59 12)(font "Arial" ))
		(text "ALUop[1..0]" (rect 21 123 80 135)(font "Arial" ))
		(line (pt 0 128)(pt 16 128)(line_width 3))
	)
	(port
		(pt 0 144)
		(input)
		(text "ALUSrc" (rect 0 0 37 12)(font "Arial" ))
		(text "ALUSrc" (rect 21 139 58 151)(font "Arial" ))
		(line (pt 0 144)(pt 16 144)(line_width 1))
	)
	(port
		(pt 0 160)
		(input)
		(text "RegWrite" (rect 0 0 46 12)(font "Arial" ))
		(text "RegWrite" (rect 21 155 67 167)(font "Arial" ))
		(line (pt 0 160)(pt 16 160)(line_width 1))
	)
	(port
		(pt 0 176)
		(input)
		(text "CPU_Clock_in" (rect 0 0 71 12)(font "Arial" ))
		(text "CPU_Clock_in" (rect 21 171 92 183)(font "Arial" ))
		(line (pt 0 176)(pt 16 176)(line_width 1))
	)
	(port
		(pt 0 192)
		(input)
		(text "FPGA_Clock_in" (rect 0 0 77 12)(font "Arial" ))
		(text "FPGA_Clock_in" (rect 21 187 98 199)(font "Arial" ))
		(line (pt 0 192)(pt 16 192)(line_width 1))
	)
	(port
		(pt 280 32)
		(output)
		(text "this_pc[31..0]" (rect 0 0 67 12)(font "Arial" ))
		(text "this_pc[31..0]" (rect 192 27 259 39)(font "Arial" ))
		(line (pt 280 32)(pt 264 32)(line_width 3))
	)
	(port
		(pt 280 48)
		(output)
		(text "next_pc[31..0]" (rect 0 0 70 12)(font "Arial" ))
		(text "next_pc[31..0]" (rect 189 43 259 55)(font "Arial" ))
		(line (pt 280 48)(pt 264 48)(line_width 3))
	)
	(port
		(pt 280 64)
		(output)
		(text "reg_rs[31..0]" (rect 0 0 62 12)(font "Arial" ))
		(text "reg_rs[31..0]" (rect 197 59 259 71)(font "Arial" ))
		(line (pt 280 64)(pt 264 64)(line_width 3))
	)
	(port
		(pt 280 80)
		(output)
		(text "reg_rt[31..0]" (rect 0 0 60 12)(font "Arial" ))
		(text "reg_rt[31..0]" (rect 199 75 259 87)(font "Arial" ))
		(line (pt 280 80)(pt 264 80)(line_width 3))
	)
	(port
		(pt 280 96)
		(output)
		(text "alu_out[31..0]" (rect 0 0 67 12)(font "Arial" ))
		(text "alu_out[31..0]" (rect 192 91 259 103)(font "Arial" ))
		(line (pt 280 96)(pt 264 96)(line_width 3))
	)
	(port
		(pt 280 112)
		(output)
		(text "mem_write_data[31..0]" (rect 0 0 112 12)(font "Arial" ))
		(text "mem_write_data[31..0]" (rect 147 107 259 119)(font "Arial" ))
		(line (pt 280 112)(pt 264 112)(line_width 3))
	)
	(drawing
		(rectangle (rect 16 16 264 208)(line_width 1))
	)
)
