/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/
/*
Copyright (C) 1991-2006 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.
*/
(header "symbol" (version "1.1"))
(symbol
	(rect 16 16 240 176)
	(text "Register_File" (rect 5 0 69 12)(font "Arial" ))
	(text "inst" (rect 8 144 25 156)(font "Arial" ))
	(port
		(pt 0 32)
		(input)
		(text "read_reg_1[4..0]" (rect 0 0 80 12)(font "Arial" ))
		(text "read_reg_1[4..0]" (rect 21 27 101 39)(font "Arial" ))
		(line (pt 0 32)(pt 16 32)(line_width 3))
	)
	(port
		(pt 0 48)
		(input)
		(text "read_reg_2[4..0]" (rect 0 0 80 12)(font "Arial" ))
		(text "read_reg_2[4..0]" (rect 21 43 101 55)(font "Arial" ))
		(line (pt 0 48)(pt 16 48)(line_width 3))
	)
	(port
		(pt 0 64)
		(input)
		(text "write_reg[4..0]" (rect 0 0 69 12)(font "Arial" ))
		(text "write_reg[4..0]" (rect 21 59 90 71)(font "Arial" ))
		(line (pt 0 64)(pt 16 64)(line_width 3))
	)
	(port
		(pt 0 80)
		(input)
		(text "write_data[31..0]" (rect 0 0 81 12)(font "Arial" ))
		(text "write_data[31..0]" (rect 21 75 102 87)(font "Arial" ))
		(line (pt 0 80)(pt 16 80)(line_width 3))
	)
	(port
		(pt 0 96)
		(input)
		(text "RegWrite" (rect 0 0 46 12)(font "Arial" ))
		(text "RegWrite" (rect 21 91 67 103)(font "Arial" ))
		(line (pt 0 96)(pt 16 96)(line_width 1))
	)
	(port
		(pt 0 112)
		(input)
		(text "CPU_Clock" (rect 0 0 57 12)(font "Arial" ))
		(text "CPU_Clock" (rect 21 107 78 119)(font "Arial" ))
		(line (pt 0 112)(pt 16 112)(line_width 1))
	)
	(port
		(pt 224 32)
		(output)
		(text "read_data_1[31..0]" (rect 0 0 92 12)(font "Arial" ))
		(text "read_data_1[31..0]" (rect 111 27 203 39)(font "Arial" ))
		(line (pt 224 32)(pt 208 32)(line_width 3))
	)
	(port
		(pt 224 48)
		(output)
		(text "read_data_2[31..0]" (rect 0 0 92 12)(font "Arial" ))
		(text "read_data_2[31..0]" (rect 111 43 203 55)(font "Arial" ))
		(line (pt 224 48)(pt 208 48)(line_width 3))
	)
	(drawing
		(rectangle (rect 16 16 208 144)(line_width 1))
	)
)
